#
BRAKES TECHNICAL DATA

BME045000000W01

Item | Specification
--- | ---
CONVENTIONAL BRAKE SYSTEM
Brake pedal | Brake pedal height | (mm {in}) | 210 {8.27} (reference value)
Brake pedal play | (mm {in}) | 7.8-12.0 {0.31-0.47}
Pedal-to-floor clearance | (mm {in}) | 113 {4.45} min.
Power brake unit | Fluid pressure (When pedal depressed at 200 N {20.4 kgf, 44.9 lbf}) | At 0 kPa {0 mmHg, 0 inHg} | 790 {8.06, 115} min.
(kPa {kgf/cm2, psi}) | At 66.7 kPa {500 mmHg, 19.7 inHg} | 8,830 {90.04, 1,280} min.
Vacuum pump | Vacuum specification | When engine speed at 1,270 rpm | 66.6 {500, 19.7}
(kPa {mmHG, inHG}) | When engine speed at 2,450 rpm | 93.3 {700, 27.6}
Front disc brake | Minimum disc pad thickness | (mm {in}) | 2.0 {0.08}
Minimum disc plate thickness | (mm {in}) | 26 {1.03}
Disc plate runout limit | (mm {in}) | 0.05 {0.002}
Rear drum brake | Maximum brake drum diameter | (mm {in}) | 255.5 {10.06}
Minimum lining thickness | (mm {in}) | 1.0 {0.04}
Clearance between shoe and drum | Automatic adjuster
Brake fluid | Type | SAE J1703 or FMVSS 116 DOT-3 or DOT-4
PARKING BRAKE SYSTEM
Parking brake lever | Lever stroke when pulled at 98 N {10 kgf, 22 lbf} | (notches) | 4-5 (no drag)