#
REAR HEATER CORE INSPECTION

BME071161410W02

1. Remove the rear heater core from the rear A/C unit.

2. Inspect for cracks, damage, and coolant leakage.

  • If any are found, replace the rear heater core.

3. Inspect for bent fins.

  • If any are bent, use a flathead screwdriver to straighten them.

4. Verify that the rear heater core inlet and outlet are not distorted or damaged.

  • If they are distorted or damaged, repair then using pliers.