#
DTC P0101 [AJ]

BME010200100201

DTC P0101 | MAF sensor inconsistent with TP sensor (lower than expected) or engine speed (greater than expected)
--- | ---
DETECTION CONDITION | • PCM monitors mass intake air flow amount when the engine is running.

  - If mass intake air flow amount is above 73 l/s for 5 s and engine speed is below 2,500 rpm with engine running and engine coolant temperature is above 70°C {158°F}, PCM determines that detected mass intake air flow amount is too high.
  - If mass intake air flow amount is below 9.3-77.0 l/s (The value depends on engine speed.) for 5 s and engine speed is above 1,000 rpm with engine running and throttle opening angle is above 50%, PCM determines that detected mass intake air flow amount is too low.

Diagnostic support note
• This is a continuous monitor (CCM).
• MIL illuminates if PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• PENDING CODE is available if PCM detects the above malfunction condition during first drive cycle.
• FREEZE FRAME DATA is available.
• DTC is stored in the PCM memory.
POSSIBLE CAUSE | • MAF sensor malfunction • Electrical corrosion in MAF RETURN circuit • Voltage drops in GND circuit

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record FREEZE FRAME DATA on repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT INPUT SIGNAL STATUS IS CONCERN INTERMITTENT OR CONSTANT • Connect WDS or equivalent to DLC-2. • Start the engine. • Access ECT, MAF, TP and RPM PIDs using WDS or equivalent. • Warm-up engine until ECT PID is above 70°C {158°F}.
• Idle engine for 5 s or more.

  Caution

  • While driving, always operate the vehicle in a safe and lawful manner.

• Drive the vehicle under the following two conditions:
Condition 1

  - TP PID: 50-87.5%
  - RPM PID: above 1,000 rpm
  - D range

Condition 2

  - TP PID: above 80%
  - RPM PID: below 2,500 rpm
  - Gear in

• Is PENDING CODE for this DTC present?
Yes
Go to next step.
No | Intermittent concern exists. Go to INTERMITTENT CONCERNS TROUBLESHOOTING procedure. (See INTERMITTENT CONCERN TROUBLESHOOTING [AJ])
4 | CHECK MAF SENSOR TERMINALS FOR ELECTRICAL CORROSION • Turn ignition switch to OFF. • Disconnect MAF sensor connector. • Check for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is any problem corrosion found? | Yes | Repair or replace suspected terminal or MAF sensor, then go to Step 6.
No | Go to next step.
5 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Disconnect PCM connector. • Check for poor connection (damaged, pulled-out pins, corrosion, etc.). • Is there any malfunction? | Yes | Repair terminal, then go to next step.
No | Go to next step.
6 | VERIFY TROUBLESHOOTING OF DTC P0101 COMPLETED • Make sure to connect all disconnected connectors. • Turn ignition switch to ON (Engine OFF). • Clear DTC from PCM memory using WDS or equivalent. • Start the engine.
• Warm-up engine until ECT PID is above 70°C {158°F}.
• Idle engine for 5 s or more.

  Caution

  • While performing the Drive Mode, always operate the vehicle in a safe and lawful manner.

• Drive the vehicle under the following two conditions:
Condition 1

  - TP PID: 50-87.5%
  - RPM PID: above 1,000 rpm
  - D range

Condition 2

  - TP PID: above 80%
  - RPM PID: below 2,500 rpm
  - Gear in

• Is PENDING CODE for this DTC present?
Yes
Replace PCM, then go to next step.
No | Go to next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [AJ].) • Is any DTC present? | Yes | Go to applicable DTC inspection. (See DTC TABLE [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See DTC TABLE [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
No | Troubleshooting completed.