#
INTAKE SHUTTER VALVE ACTUATOR INSPECTION [MZR-CD (RF Turbo)]

BME011620132W01

1. Disconnect the vacuum hose from the intake shutter valve actuator.

2. Connect a vacuum pump to port A.

3. Apply vacuum and verify that the rod moves.

  • If the rod does not move, replace the intake manifold.

Specification

Vacuum kPa {mmHg, inHg} | Rod movement
--- | ---
Below -20 {-150, -5.9} | Starts to move
Above -66 {-495, -19} | Fully pulled

4. Connect a vacuum pump to port A and B.

5. Apply vacuum and verify that the rod moves.

  • If the rod does not move, replace the intake manifold.

Specification

Vacuum kPa {mmHg, inHg} | Rod movement
--- | ---
Above -69.4 {-520, -21} | Fully pulled