#
FRONT TWEETER REMOVAL/INSTALLATION

BME092051050201

1. Disconnect the negative battery cable.

2. Remove the A-pillar trim.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Front tweeter F Front Tweeter Removal Note
2 | Connector

## Front Tweeter Removal Note

1. Insert your hand between the A-pillar and the dashboard, then compress the tabs of the front tweeter from the back of the dashboard.