#
OIL PUMP REMOVAL/INSTALLATION [AJ]

BME011114100202

  Caution

  • Position the hose clamp in the original location on the hose, and squeeze the clamp lightly with large pliers to ensure a good fit.
  • After radiator cowling installation, rotate the cooling fan by hand and verify that the fan blade does not touch the radiator cowling. If the fan touches the cowling, adjust the radiator cowling mounting position.

1. Disconnect the negative battery cable.

2. Drain the engine oil. (See ENGINE OIL REPLACEMENT.)

3. Remove the oil pan. (See OIL PAN REMOVAL/INSTALLATION [AJ].)

4. Remove the timing chain. (See TIMING CHAIN REMOVAL/INSTALLATION [AJ].)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Refill the engine with the specified type and amount of the engine oil. (See ENGINE OIL REPLACEMENT.)

8. Start the engine and inspect for engine oil leakage.

9. Inspect the oil pressure. (See OIL PRESSURE INSPECTION [AJ].)

1 | Oil strainer (See Oil Strainer Installation Note.)
2 | Oil pump (See Oil Pump Removal Note.) (See Oil Pump Installation Note.)

## Oil Pump Removal Note

1. Loosen the oil pump bolts in the order as shown in the figure.

## Oil Pump Installation Note

1. Tighten the oil pump bolts in the order as shown in the figure.

## Oil Strainer Installation Note

1. Tighten the oil strainer bolts.

Tightening torque

  8-12 N·m {82-122 kgf·cm, 71-106 in·lbf}

2. Tighten the new oil strainer stay nut to 15.0 N·m {153 kgf·cm, 133 in·lbf}, then tighten it further 45° using the SST.