#
THROTTLE POSITION (TP) SENSOR INSPECTION [L3]

BME014018910201

  Note

  • Perform the following inspection only when directed.

## Resistance Inspection

1. Perform the following test only when directed.

  • If as specified but TP PID value is out of specification, inspect resistance of TP sensor.
  • If not as specified, inspect the following:

  - Accelerator cable free play (See ACCELERATOR CABLE INSPECTION [L3].)

2. Disconnect the TP sensor connector.

3. Verify that the resistance between TP sensor terminals A and B changes smoothly while opened and closed the throttle valve slowly.

  • If not verified, replace TP sensor.

4. Measure the resistance between TP sensor terminals A and C using an ohmmeter.

  • If not as specified, replace the TP sensor.
  • If as specified, but TP PID value is out of specification, perform the "Circuit Open/Short Inspection".

Specification

  3.2-4.8 kilohms

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [L3].)

2. Inspect the following wiring harnesses for open or short. (Continuity check)

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the harness.
  - TP sensor terminal A (harness-side) and PCM terminal 2H (harness-side)
  - TP sensor terminal B (harness-side) and PCM terminal 2A (harness-side)
  - TP sensor terminal C (harness-side) and PCM terminal 2K (harness-side)

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the harness.
  - TP sensor terminal C (harness-side) and power supply
  - TP sensor terminal C (harness-side) and body GND
  - TP sensor terminal B (harness-side) and power supply
  - TP sensor terminal B (harness-side) and body GND
  - TP sensor terminal A (harness-side) and power supply