#
CRUISE ACTUATOR REMOVAL/INSTALLATION

BME012066310201

1. Disconnect the negative battery cable.

2. Remove the engine cover.

3. Remove in the order indicated in the table.

1 | Cover
2 | Actuator cable (See ACTUATOR CABLE REMOVAL.) (See ACTUATOR CABLE INSTALLATION.)
3 | Nut
4 | Connector
5 | Screw
6 | Bracket
7 | Short cord (See Short Cord Installation Note)
8 | Cruise actuator

4. Install in the reverse order of removal.

## Short Cord Installation Note

1. Install the connector of the short cord to the bracket.