#
DTC P0606 [MZR-CD (RF Turbo)]

BME010200600W03

DTC P0606 | PCM malfunction
--- | ---
DETECTION CONDITION | • PCM does not read DTC from output devices.
POSSIBLE CAUSE | • PCM internal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | - | - | Replace PCM and reprogram immobilizer system. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].) (See IMMOBILIZER SYSTEM REPROGRAM PROCEDURE.)