#
TROUBLESHOOTING INDEX

BME090369000W02

No. | TROUBLESHOOTING ITEM | DESCRIPTION | PAGE
--- | --- | --- | ---
1 | One or more on-board diagnostic functions inoperative. | • Malfunction in hazard warning light system (except vehicle with theft-deterrent system), horn system (Australian specs.) door lock linkage system, or driver's door key cylinder switch system. | (See NO. 1 ONE OR MORE ON-BOARD DIAGNOSTIC FUNCTIONS INOPERATIVE)
2 | All on-board diagnostic functions inoperative. | • Malfunction in keyless unit power supply circuit, door switch circuit or keyless unit ground circuit. | (See NO. 2 ALL ON-BOARD DIAGNOSTIC FUNCTIONS INOPERATIVE)