#
SECOND-ROW BUCKLE REMOVAL/INSTALLATION

BME081157720201

## TYPE A

1. Remove the second-row seat.

2. Remove the side cover.

3. Remove as indicated in the table.

4. Install in the reverse order of removal.

1 | Second-row buckle

## TYPE B

1. Remove the seat cushion. (See SECOND-ROW SEAT DISASSEMBLY/ASSEMBLY.)

2. Remove the bolt, and then remove the second-row buckle.

3. Install in the reverse order of removal.