#
VACUUM SWITCH REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME041166390W02

1. Remove in the order indicated in the table.

1 | Connector
2 | Vacuum switch (See Vacuum Switch Installation Note)

2. Install in the reverse order of removal.

## Vacuum Switch Installation Note

  Caution

  • Do not apply sealant to the lip of the vacuum switch as it may cause a malfunction to occur.

1. apply sealant to the area shown of the new vacuum switch.