#
DIAGNOSTIC MONITORING TEST RESULTS [L3]

BME010200000W05
• The purpose of this test mode is to confirm the result of the OBD monitor diagnostic test results. The result values stored when a particular monitored item is completed are displayed. If the monitored item is not completed, initial value is displayed.

TEST ID | Description | Related system
--- | --- | ---
10:01:01*1 | Rich to lean sensor threshold voltage | HO2S
10:01:02*1 | Lean to rich sensor threshold voltage
10:01:03*1 | Low sensor voltage for switching time calculation
10:01:04*1 | High sensor voltage for switching time calculation
10:01:05*1 | Rich to lean sensor switching time
10:01:06*1 | Lean to rich sensor switching time
10:01:0A*1 | Rich to lean sensor threshold voltage
10:21:80*1 | Front and rear HO2S switching time ratio | TWC
10:31:83*2 | EGR flow test | EGR

  *1 :
European (L.H.D. U.K.) specs.
  *2 :
Except for European (L.H.D. U.K.) specs.