#
FRONT A/C UNIT REMOVAL/INSTALLATION

BME071161130201

1. Disconnect the negative battery cable.

2. Drain the engine coolant.

3. Evacuate the refrigerant from the system. (See REFRIGERANT CHARGING.)

  Caution

  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise will occur. Always immediately plug open fittings after removing any refrigeration cycle parts to keep moisture or foreign material out of the cycle.

4. Remove the dashboard. (See DASHBOARD REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Perform the refrigerant system performance test.

ENGINE ROOM

PASSENGER ROOM

1 | Front heater hose (See Heater Pipe and Hose Component Installation Note)
2 | Front cooler pipe No.3 (See Refrigerant Lines Removal Note) (See Refrigerant Lines Installation Note)
3 | Air duct
4 | Front A/C unit