#
SUSPENSION FEATURES

BME020001013T01

Improved rigidity | • Torsion beam axle type rear suspension adopted • Front transverse member adopted
Improved straight-ahead handling and driving comfort | • Separated input type shock absorber mount adopted • Low-pressure gas charged shock absorber adopted
Improved marketability | • Adhesive-type balance weights adopted (aluminum alloy wheels)
Environmental consideration | • Steel balance weights adopted to reduce the use of lead