#
VALVE, VALVE SPRING, VALVE SEAL, VALVE GUIDE CONSTRUCTION [L3]

BME011012111T02
• The valves are heat-resistant steel. There are two intake valves, two exhaust valves per cylinder.

VALVE SPEC.

ITEM | L3
--- | ---
valve full length | (mm {in}) | Intake valve: About 101.6 {4.000} Exhaust valve: About102.6 {4.039}
Intake valve umbrella diameter | (mm {in}) | About 35 {1.38}
Exhaust valve umbrella diameter | (mm {in}) | About 30 {1.18}
Stem diameter | (mm {in}) | Intake valve: About 5.5 {0.22} Exhaust valve: About 5.5 {0.22}

• The intake valve and the exhaust valve are treated with the tufftride process to improve abrasion resistance.
• The valve spring is an uneven outer dimension type. It has been improved by reducing the size of the upper seat.
• The valve guide is made of the sintered alloy to improve abrasion resistance.
• The valve seat is integrated with the lower valve spring seat to simplify the unit and improve its serviceability.

1 | Valve keeper
2 | Upper valve spring seat
3 | Valve spring
4 | Valve seal
5 | Valve guide
6 | Valve