#
GENERATOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME011718300W03

  Warning

  • When the battery cables are connected, touching the vehicle body with generator terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the battery before performing the following operation.

  Caution

  • The generator can be damaged by the heat from the exhaust manifold. Make sure the generator duct and the generator heat insulator are installed securely.

1. Disconnect the negative battery cable.

2. Remove the splash shield.

3. Remove the A/C compressor with hose and pipe still connected.

4. Remove the cooling fan component. (See COOLING FAN MOTOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

5. Remove the drive belt. (See DRIVE BELT REPLACEMENT [MZR-CD (RF Turbo)].)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

.

1 | Terminal B wire
2 | Connector
3 | Generator
4 | Pulley (See Pulley Disassembly/Assembly Note.)

## Pulley Disassembly/Assembly Note

1. Disassemble/assemble the pulley using the SST.

Tightening torque

  60-85 N·m {6.1-8.7 kgf·m, 45-62 ft·lbf}