#
DTC 00 ERR04 OR 00:ER04

BME090266900W17

DTC 00 ERR04 or 00:Er04 | Cassette tape
DETECTION CONDITION |

  Note

  • When error occurs, error message "CHECK TAPE" is displayed in the LCD.

• Cassette tape is worn out.
POSSIBLE CAUSE | • Tape wear • Cassette deck malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CASSETTE TAPE • Inspect condition of cassette tape where error has occurred. • Is cassette tape okay? | Yes | Go to next step.
No | Replace cassette tape, then go to next step.
2 | INSPECT CASSETTE DECK • Clear DTC. • Insert cassette tape with no defect. • Play cassette tape for 20 seconds or more. • Start on-board diagnostic test mode.
• Is DTC 00 ERR04 or 00:Er04 displayed?
Yes
Replace cassette deck.
No | Troubleshooting completed.