#
IDLE AIR CONTROL (IAC) OUTLINE [L3]

BME014000000T07
• The IAC for Mazda MPV has been adopted or changed the following parts.

  - Add the MAP factor to the feedback correction.
  - Target engine speed is different caused to much the vehicle characteristics.

## Target Engine Speed

Condition | Engine speed (rpm)*1
--- | ---
No load | 650
E/L is operating. | 650
P/S is operating. | 700
A/C is operating.*2 | 700

  *1 :
Excludes temporary idle speed drop just after the electrical loads are turned on.
  *2 :
A/C switch and fan switch are on.