#
FRONT CLIMATE CONTROL UNIT WIRE ADJUSTMENT

BME074061335W01

## Air Mix Wire

1. Set the temperature control dial at MAX HOT.

2. Set the air mix link to MAX HOT in the direction shown by the arrow and insert a screwdriver at the set hole.

3. Connect the air mix wire to air mix link.

4. Clamp the air mix wire to the wire clamp.

5. Verify that the temperature control dial moves its full stroke.

## Airflow Mode Wire

1. Set the airflow mode control dial at VENT.

2. Set the airflow mode link to VENT in the direction shown by the arrow and insert a screwdriver at the set hole.

3. Connect the airflow mode wire to airflow mode link.

4. Clamp the airflow mode wire to the wire clamp.

5. Verify that the airflow mode control dial moves its full stroke.