#
TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [FN4A-EL]

BME051719200204

1. Disconnect the negative battery cable.

2. Remove the splash shield.

  Caution

  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to spill water or foreign material on the connector when disconnecting it.

3. Remove the clip and disconnect the selector cable.

  Caution

  • Do not use an impact wrench. Hold the manual shaft lever when removing the manual shaft nut, otherwise the transaxle may be damaged.

4. Rotate the manual shaft fully to the converter housing side, then return two notches to set the N position.

5. Disconnect the TR switch connector.

6. Loosen the TR switch mounting bolts.

7. Adjust the TR switch to the point where there is continuity between terminals D and I.

8. Tighten the TR switch mounting bolts.

Tightening torque

  8-11 N·m {82-112 kgf·cm, 71-97 in·lbf}

9. Shift the selector lever to the P position.

10. Turn the manual shaft lever to the P position.

11. Connect the TR switch connector.

12. Install the clip to the selector cable as shown in the figure.

13. Connect the selector cable.

14. Install the splash shield.

15. Connect the negative battery cable.

16. Inspect operation of the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FN4A-EL].)

  • If there is any malfunction, readjust the TR switch. (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [FN4A-EL].)