#
AUTOMATIC TRANSAXLE SHIFT MECHANISM OUTLINE

BME051846010T01
• Remote column shifting operates a push-pull cable.
• The selector lever is attached to the steering column and operates on the same axis as the steering shaft. The selector lever, which is made of resin, has an O/D OFF switch installed on its end.
• A key interlock device and a shift lock device have been adopted. A shift-lock release lever, mounted on the steering column cover, makes operation of the vehicle possible even if the battery becomes discharged and the shift lock cannot be unlocked.