#
POWER WINDOW SUBSWITCH REMOVAL/INSTALLATION

BME091266370W01

## Passenger's Side

1. Disconnect the negative battery cable.

2. Remove the front door trim.

3. Push out the clip from behind the front door trim, and remove the switch panel.

4. Remove the screws and the power window subswitch.

5. Install in the reverse order of removal.

## Rear

1. Disconnect the negative battery cable.

2. Remove the hook by inserting a tape-wrapped flathead screwdriver between the switch and the rear door trim.

3. Disconnect the connector, and remove the power window subswitch.

4. Install in the reverse order of removal.