#
CYLINDER HEAD (I) DISASSEMBLY

BME011002000618

1. Disassemble in the order indicated in the table.

1 | No.3 engine mount bracket
2 | Water outlet
3 | Dipstick
4 | Bypass pipe
5 | Cylinder head cover
6 | Fuel injection pipe
7 | Fuel injection pipe
8 | Common rail
9 | EGR water cooler
10 | Injection pump
11 | Intake manifold
12 | Injection pump bracket
13 | Nozzle seal
14 | Side wall
15 | Injection nozzle bracket
16 | Injection nozzle
17 | Rocker arm and rocker arm shaft (SeeRocker Arm and Rocker Arm Shaft Disassembly Note)
18 | Rocker bridge
19 | Camshaft
20 | Breather pipe

## Rocker Arm and Rocker Arm Shaft Disassembly Note

1. Inspect the camshaft end play.

(See CAMSHAFT END PLAY INSPECTION)

2. Inspect the camshaft oil clearance.

(See CAMSHAFT OIL CLEARANCE INSPECTION)

3. Loosen the bolts in two or three steps in the order shown.