#
SIMULATION TEST [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed))

BME010200000T24
• The simulation test items for the fuel and emission control systems are as shown in the table below.

Simulation item table

×: Applicable
-: Not applicable

Item | Applicable component | Unit/condition | Test condition | PCM terminal
--- | --- | --- | --- | ---
KOEO | KOER
ACCS | A/C relay | On/Off | × | × | 47
ALTF | Generator field coil control duty value | On/Off | - | × | 63
ARPMDES | Target engine speed | RPM | × | × | -
BARO/EGR | EGR boosst sensor solenoid valve | On/Off | × | × | 93
EVAPCP | Purge solenoid valve duty value | % | × | × | 85
FAN_DUTY | Fan control duty value | % | × | × | 69
FP | Fuel pump relay | On/Off | × | × | 95*1, 67*2
FUELPW1 | Fuel injector duration | % | - | × | -
FUELPW2 | Fuel injector duration | % | - | × | -
GENVDSD | Target generator voltage | V | - | × | -
HTR11 | HO2S (front RH) heater | On/Off | × | × | 83
HTR12*3 | HO2S (rear RH) heater | On/Off | × | × | 57
HTR21 | HO2S (front LH) heater | On/Off | × | × | 84
HTR22*3 | HO2S (rear LH) heater | On/Off | × | × | 58
IAC | IAC valve | % | × | × | 88
IMCC | IMCC actuator | On/Off | × | × | 97
INJ_1 | Fuel injector No.1 | Off | - | × | 76
INJ_2 | Fuel injector No.2 | Off | - | × | 50
INJ_3 | Fuel injector No.3 | Off | - | × | 75
INJ_4 | Fuel injector No.4 | Off | - | × | 49
INJ_5 | Fuel injector No.5 | Off | - | × | 74
INJ_6 | Fuel injector No.6 | Off | - | × | 48
SEGRP | EGR valve | (Step) | × | × | 72, 73, 98, 99
test | Test mode | On/Off | × | × | -

  *1 :
With immobilizer system
  *2 :
Without immobilizer system
  *3 :
With HO2S rear model