#
CONTROL SYSTEM DIAGRAM [AJ]

BME014000000T54

1 | IAT sensor
2 | MAF sensor
3 | TP sensor
4 | ECT sensor
5 | CMP sensor
6 | Knock sensor
7 | CKP sensor
8 | HO2S (front, RH) (integrated with front HO2S heater)
9 | HO2S (front, LH) (integrated with front HO2S heater)
10 | HO2S (rear, RH) (integrated with rear HO2S heater) (European (L.H.D.) specs.)
11 | HO2S (rear, LH) (integrated with rear HO2S heater) (European (L.H.D.) specs.)
12 | IAC valve
13 | Fuel injector
14 | Pressure regulator (equipped with fuel pump)
15 | Fuel filter (low-pressure)
16 | Fuel pump body
17 | Fuel tank
18 | Fuel filter (high-pressure)
19 | Purge solenoid valve
20 | Catch tank
21 | Charcoal canister
22 | Check valve
23 | EGR valve
24 | BARO sensor (European (L.H.D.) specs.), EGR boost sensor (Australian, General (L.H.D. R.H.D.) specs.)
25 | EGR boost sensor solenoid valve (used for Australian, General (L.H.D. R.H.D.) specs.)
26 | Rollover valve
27 | WU-TWC
28 | TWC
29 | Pulsation damper
30 | Ignition coil No.1
31 | Ignition coil No.2
32 | Ignition coil No.3
33 | Ignition coil No.4
34 | Ignition coil No.5
35 | Ignition coil No.6
36 | PCM
37 | Generator
38 | PCV valve
39 | Intake manifold communication control (IMCC) actuator
40 | To PCM