#
DIFFERENTIAL DISASSEMBLY

BME051527100302

1. Disassemble in the order indicated in the table.

1 | Bolts
2 | Ring gear
3 | Screw
4 | Differential cover
5 | Bearing (See Bearing Disassembly Note.)
6 | Speedomter driver gear
7 | Thrust washer
8 | Side gear
9 | Roll pin
10 | Pinion shaft
11 | Pinion carrier
12 | Pinion gear
13 | Thrust washer
14 | Side gear
15 | Thrust washer
16 | Gear case

## Bearing Disassembly Note

1. Remove the bearing (speedometer drive gear side) from the gear case using the SSTs.

2. Remove the bearing (differential cover side) from the differential cover using the SSTs.