#
COOLING FAN MOTOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME011215025W04

1. Disconnect the negative battery cable.

2. Remove the transverse member. (See TRANSVERSE MEMBER REMOVAL/INSTALLATION.)

3. Remove the engine mount member.

4. Remove the radiator hose. (See RADIATOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

5. Remove the No.2 engine mount.

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

1 | Fan control module connectors
2 | Fan control module
3 | Radiator bracket
4 | Fan motor component
5 | Main fan
6 | Additional fan
7 | Main fan motor
8 | Additional fan motor