#
CORRECTION PROCEDURE [MZR-CD (RF Turbo)]

BME011002000W08

  Note

  • Perform each procedure by selecting the corresponding menu on the WDS screen. These procedures appear when "Powertrain" in the "Toolbox tab" is selected.

## Correction after Parts Installation

  Note

  • Perform this procedure after replacing the PCM and/or fuel injectors.

1. Perform "Engine Tune-up Preparation". (See ENGINE TUNE-UP PREPARATION [MZR-CD (RF Turbo)].)

2. Perform "Correction after Parts Installation" using the WDS or equivalent.

## Injection Amount Correction

  Note

  • Perform this procedure at the recommended interval as described under "Fuel injection system" in "SCHEDULED MAINTENANCE."

1. Perform "Engine Tune-up Preparation". (See ENGINE TUNE-UP PREPARATION [MZR-CD (RF Turbo)].)

2. Perform "Injection Amount Correction" using the WDS or equivalent.

## MAF Correction

  Note

  • Perform this procedure after replacing the MAF/IAT sensor or at the recommended interval as described under "E.G.R. system" in "SCHEDULED MAINTENANCE."

1. Perform "Engine Tune-up Preparation". (See ENGINE TUNE-UP PREPARATION [MZR-CD (RF Turbo)].)

2. Perform "MAF Correction" using the WDS or equivalent.