#
SIDE SILL PANEL AND END PLATE INSTALLATION

BME098070270B02

1. When joining the new and old parts, temporarily install and fit the new part in position, measure each dimension according to the body dimension drawing, then adjust the position to align it to the standard dimension.

2. After trial-fitting new parts, make sure the related parts fit properly.

3. Drill holes for plug welds before installing new parts.