#
CAMSHAFT CONSTRUCTION [AJ]

BME011012420T04
• A steel camshaft has been adopted.
• A hollow assembly type camshaft with a press fit cam lobe has been adopted to improve weight reduction.
• The front of the camshaft sprockets have been separately marked RH, LH, IN and EX to prevent mis-assembly.
• The rear end of the of the intake camshaft (LH) is engaged with the water pump pulley.

Valve timing

1 | Valve timing
2 | TDC
3 | BTDC 4°
4 | ATDC 12°
5 | ABDC 4°
6 | BDC
7 | BBDC 56°
8 | Intake camshaft
9 | Cam robe
10 | Sprocket
11 | Mark
12 | Exhaust camshaft
13 | Cam robe