#
OIL SEAL REPLACEMENT [FN4A-EL]

BME051727238201

1. Drain the ATF. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [FN4A-EL].)

  Caution

  • The oil seal is easily damaged by the sharp edges of the drive shaft splines. Do not allow the splines contact the oil seal.

2. Remove the drive shaft and joint shaft. (See DRIVE SHAFT (L3) REMOVAL/INSTALLATION.) (See JOINT SHAFT (L3) REMOVAL/INSTALLATION.)

3. Remove the oil seal.

4. Using the SST and a hammer, tap a new oil seal in evenly until the SST contacts the transaxle case.

5. Coat the lip of the oil seal with transaxle oil.

6. Install the drive shaft and joint shaft. (See DRIVE SHAFT (L3) REMOVAL/INSTALLATION.) (See JOINT SHAFT (L3) REMOVAL/INSTALLATION.)

7. Add ATF to the specified level. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [FN4A-EL].)

8. Perform the mechanical system test. (See MECHANICAL SYSTEM TEST [FN4A-EL].)