#
SLIDING DOOR CIRCUIT CONTACT INSPECTION

BME091100104202

## Door Side

1. Disconnect the sliding door circuit contact connector.

2. Inspect for continuity between the sliding door circuit contact terminals using an ohmmeter.

  • If not as specified, replace the sliding door circuit contact.

## Body Side

1. Disconnect the sliding door circuit contact connector.

2. Inspect the sliding door circuit contact terminals for continuity using an ohmmeter.

  • If not as specified, replace the sliding door circuit contact.