#
BRAKES SPECIFICATIONS

BME040001020103

Item | Specification
--- | ---
Brake pedal | Type | Suspended
Pedal lever ratio | 4.1
Max. stroke | (mm {in}) | 125 {4.92}
Master cylinder | Type | Tandem (with level sensor)
Cylinder diameter | (mm {in}) | 25.40 {1.00}
Front disc brake | Type | Ventilated disc
Cylinder bore | (mm {in}) | 42.85 {1.687} × 2
Pad dimensions (area × thickness) | 5,850 {9.36} × 10.5 {0.413}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | 274 {10.8} × 28 {1.1} : L3, AJ 296 {11.7} × 28 {1.1} : MZR-CD (RF Turbo)
(mm {in})
Rear disc brake | Type | Ventilated disc
Cylinder bore | (mm {in}) | 38.10 {1.50}
Pad dimensions (area × thickness) | 2,900 {4.64} × 11.0 {0.43}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | 286 {11.3} × 18 {0.7}
(mm {in})
Power brake unit | Type | Vacuum multiplier, tandem diaphragm
Diameter | (mm {in}) | 213.4 + 240.2 {8.40 + 9.46}
Parking brake | Type | Mechanical two-rear-wheel control
Operation system | Center lever
Drum brake type | Servo type
Lining width | (mm {in}) | 22.5 {0.89}
Drum inner diameter | (mm {in}) | 190 {7.48}
Shoe clearance adjustment | Manual adjuster
Braking force control device | Type | EBD
Brake fluid | Type | European (L.H.D. U.K.) specs: SAE J1703, FMVSS116 DOT-3 OR DOT-4 Except European (L.H.D. U.K.) specs: SAE J1703, FMVSS116 DOT-3