#
TRANSAXLE OIL REPLACEMENT [A65M-R]

BME051527001204

1. Remove the drain plug with the gasket.

2. Drain the oil into a suitable container.

3. Install a new gasket and the drain plug.

Tightening torque

  30.0-39.0 N·m {3.06-3.98 kgf·m, 22.1-28.8 in·lbf}

4. Remove the filler plug with gasket and add the specified amount and type of oil through the filler plug hole until the level reaches the bottom of the filler plug hole.

Oil grade

  API Service GL-4 or GL-5

Oil viscosity

  SAE 75W-90

Capacity (approx. quantity)

  2.30 L {2.43 US qt, 2.02 lmp qt}

5. Install a new gasket and the filler plug.

Tightening torque

  30.0-39.0 N·m {3.06-3.98 kgf·m, 22.1-28.8 in·lbf}