#
DTC P0183 [MZR-CD (RF Turbo)]

BME010200100W34

DTC P0183 | Fuel temperature sensor circuit high input
--- | ---
DETECTION CONDITION | • PCM monitors input voltage from fuel temperature sensor while engine is running. If input voltage from fuel temperature sensor is above 5.0 V, PCM determines fuel temperature sensor circuit high input.
POSSIBLE CAUSE | • Fuel temperature sensor malfunction • Connector or terminal malfunction • Short to power circuit in wiring between fuel temperature sensor terminal A and PCM terminal 35 • Open circuit in wiring between fuel temperature sensor terminal A and PCM terminal 35
• Open circuit in wiring between fuel temperature sensor terminal B and PCM terminal 91
• PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to next step.
No | Go to next step.
2 | INSPECT POOR CONNECTION OF FUEL TEMPERATURE SENSOR CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to Step 7.
No | Go to next step.
3 | INSPECT FUEL TEMPERATURE SENSOR SIGNAL CIRCUIT FOR SHORT TO POWER • Turn engine switch to ON (Engine OFF). • Inspect voltage between fuel temperature sensor terminal A and body GND. • Is voltage below 1.0 V? | Yes | Go to next step.
No | Repair or replace harness for short to power, go to Step 7.
4 | INSPECT FUEL TEMPERATURE SENSOR • Inspect fuel temperature sensor. (See FUEL TEMPERATURE SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Repair supply pump, go to Step 7. (See SUPPLY PUMP INSPECTION [MZR-CD (RF Turbo)].)
No | Go to next step.
5 | INSPECT POOR CONNECTION OF PCM CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to Step 7.
No | Go to next step.
6 | INSPECT FUEL TEMPERATURE SENSOR CIRCUIT FOR OPEN • Turn engine switch to OFF. • Inspect continuity between following harnesses:

  - Fuel temperature sensor terminal A and PCM terminal 35.
  - Fuel temperature sensor terminal B and PCM terminal 91.

• Is there continuity?
Yes
Go to next step.
No | Repair or replace harness for open, go to next step.
7 | VERIFY TROUBLESHOOTING OF DTC P0183 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Replace PCM, go to next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].) • Is there any DTC present? | Yes | Go to applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.