#
NO.11 SHIFT POINT IS HIGH OR LOW [FN4A-EL]

BME050301030215

11 | Shift point is high or low
DESCRIPTION | • Shift point considerably different from automatic shift diagram. • Shift delays when accelerating. • Shift occurs quickly when accelerating and engine speed does not increase.
POSSIBLE CAUSE | • If the transaxle does not shift abnormally, there is a malfunction of the input signal to the TP sensor, input/turbine speed sensor, or vehicle speed sensor (including sensor GND). • If the engine speed is high or low, regardless normal of shifting, inspect the tachometer.
• Verify that the output signal of the TP sensor changes linearly.