#
ENGINE OIL LEVEL INSPECTION

BME011114001201

1. Position the vehicle on level ground.

2. Warm up the engine to normal operating temperature.

3. Stop the engine and wait for 5 min.

4. Verify that the oil level is between the MIN and MAX marks (AJ and L3 engine models), L and F marks (MZR-CD (RF-Turbo) engine model) on the dipstick and inspect the engine oil condition.

  • If the oil level is below the MIN mark, add genuine motor oil.
  • If necessary, replace with genuine engine oil.