#
PARKING BRAKE (LEVER TYPE) REMOVAL/INSTALLATION

BME041244300W04

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

  Caution

  • There are two types of parking brakes. Before installing the parking brake, comfirm the type and install them in the corresponding order.

3. Adjust the parking brake stroke. (See PARKING BRAKE (LEVER TYPE) ADJUSTMENT.)

.

1 | Cover
2 | Cover
3 | Adjusting nut
4 | Parking brake switch
5 | Parking brake lever
6 | Front cable cover (See Front Cable Cover Removal Note)
7 | Front cable and equalizer
8 | Clip
9 | Brake drum
10 | Leading shoe
11 | Parking brake cable

## Front Cable Cover Removal Note

1. Remove the front seats. (See FRONT SEAT REMOVAL/INSTALLATION.)

2. Remove the front scuff plates. (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

3. Remove the console lower cover. (See CONSOLE LOWER COVER REMOVAL/INSTALLATION.)

4. Remove the B-pillar lower trims. (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

5. Turn the floor covering over until the front cable cover appears.