#
POWER STEERING OIL PUMP (AJ) DISASSEMBLY/ASSEMBLY

BME061232650205

  Note

  • The following procedure is for replacement of the O-ring and oil seal only. Replace the pump component if other repairs are necessary.

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Power steering oil pump component (See Power Steering Oil Pump Component Disassembly Note.)
2 | Suction pipe
3 | O-ring
4 | Pressure switch component
5 | Connector
6 | O-ring
7 | Control valve
8 | Spring
9 | Rear pump body (See Rear Pump Body Assembly Note.)
10 | Gasket
11 | Pin
12 | Cam ring (See Cam Ring Assembly Note.)
13 | Rotor
14 | Vane (See Vane Assembly Note.)
15 | Side plate
16 | O-ring
17 | Snap ring
18 | Shaft component (See Shaft Component Assembly Note.)
19 | Oil seal
20 | Front pump body

## Power Steering Oil Pump Component Disassembly Note

1. Secure the power pressure oil pump using the SST.

  Caution

  • Use the SST to prevent damage to the pump when securing it in a vise.

## Shaft Component Assembly Note

1. Assemble the shaft component using the SST.

## Vane Assembly Note

1. Place the vanes in the rotor with the rounded edges contacting the cam.

## Cam Ring Assembly Note

1. Install the cam ring in the front pump body with the mark facing upward.

## Rear Pump Body Assembly Note

1. After installing the rear body, manually turn the shaft to verify that it rotates smoothly.