#
SECONDARY SHAFT END PLAY ADJUSTMENT

BME051501029M03

  Note

  • Adjust the secondary shaft end play by measuring clearance M between the transaxle case and the secondary shaft rear bearing, and selecting a secondary shaft bearing adjustment shim.
  • Calculate adjustment shim thickness P as defined below to adjust the secondary shaft bearing end play to standard.

  Standard: 0.00-0.06 mm {0.0000-0.0024 in}
  Dimension P = M - end play
  P: adjustment shim thickness
  M: transaxle case contact face and secondary shaft rear bearing contact

Adjustment shim thickness

(mm {in})

0.40 {0.016} (A65M-R) | 0.60 {0.024} | 0.80 {0.031} | 1.00 {0.039}
0.44 {0.017} (A65MX-R) | 0.64 {0.025} | 0.84 {0.033} | 1.04 {0.041}
0.48 {0.019} | 0.68 {0.027} | 0.88 {0.035} | 1.08 {0.043}
0.52 {0.020} | 0.72 {0.028} | 0.92 {0.036} | -
0.56 {0.022} | 0.76 {0.030} | 0.96 {0.038} | -

1. Install the secondary shaft component to the clutch housing.

2. Install the snap ring to the transaxle case.

3. Attach the transaxle case to the clutch housing, and temporarily install installation bolts. Temporarily attach the snap ring to the secondary shaft rear bearing.

4. Set a dial gauge to the secondary shaft rear bearing through the snap ring installation hole.

5. While expanding the snap ring, lift the secondary shaft component through the control component installation hole until it contacts the transaxle case.

6. Release the secondary shaft component so that it moves back down and the snap ring resets to the secondary shaft rear bearing. Dimension M is the measured distance that the secondary shaft component moves.

  Note

  • Select only one adjustment shim.

7. Install the selected primary shaft rear bearing adjustment shim in the primary shaft component.