#
NO.2 MIL ILLUMINATES [L3]

BME010300000W04

2 | MIL ILLUMITATES
--- | ---
DESCRIPTION | MIL is illuminated incorrectly.
POSSIBLE CAUSE | • PCM illuminates for emission-related concern (DTC is stored in PCM) • Instrument cluster malfunction

  Note

  • If MIL blinks at steady rate, misfire condition could possibly exist.

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Connect WDS or equivalent to DLC-2. Retrieve any DTC. Are there DTC displayed? | Yes | DTC is displayed: • Go to appropriate DTC test.
No | No DTC is displayed: • Inspect instrument cluster operation. (See INSTRUMENT CLUSTER INSPECTION.)
2 | Verify test results. • If okay, return to diagnostic index to service any additional symptoms. • If malfunction remains, replace PCM.