#
MASTER CYLINDER DISASSEMBLY/ASSEMBLY

BME041143400202

  Caution

  • If the master cylinder body is damaged, replace the unit as a component. When securing the master cylinder in a vise, tighten only the flange of the master cylinder.

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Cap
2 | Filter
3 | Screw
4 | Reservoir
5 | Joint bushing
6 | Fluid level sensor
7 | Snap ring
8 | Spacer
9 | Piston guide
10 | O-ring
11 | Cup
12 | Primary piston stopper
13 | Primary piston
14 | Stop pin (See Stop Pin Assembly Note)
15 | O-ring
16 | Secondary piston
17 | Master cylinder body

## Stop Pin Assembly Note

1. Install the secondary piston with the piston hole

facing the stop pin.

2. Install the new O-ring onto the stop pin.

3. Install the stop pin.

Tightening torque

  6.9-9.8 N·m {71-99 kgf·cm, 62-86 in·lbf}

4. Push and release the secondary piston assembly to verify that it si held by the stop pin.