#
DTC P0756 (ISRAELI SPECS.) [JA5A-EL]

BME050218901218

DTC P0756 | Shift solenoid B malfunction (stuck off)
--- | ---
DETECTION CONDITION | • If the difference between the actual gear ratio and the gear ratio set in the TCM is large, the TCM determines that there is a malfunction. Diagnostic support note: • This is a continuous monitor (CCM). • The MIL illuminates if the TCM detects the above malfunction condition.
• PENDING CODE is not available.
• FREEZE FRAME DATA is available.
• The HOLD indicator light does not flashes.
• The DTC is stored in the TCM memory.
POSSIBLE CAUSE | • Shift solenoid B malfunction • Stuck shift valve B • TCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME PID DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Bulletins and/or on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT FOR DTC • Turn the ignition switch to the ON position (engine off). • Inspect the DTC. • Is the DTC output? | Yes | Follow the applicable DTC inspection procedure.
No | Go to the next step.
4 | INSPECT ATF CONDITION • Turn the ignition switch to the LOCK position. • Inspect the ATF condition.

  - Transparent red: Normal
  - Milky: Water mixed in fluid
  - Reddish brown: Deteriorated ATF

• Is it normal?
(See Automatic Transaxle Fluid (ATF) Condition Inspection.)
Yes
Replace the control valve body, then go to the next step.
No | If the ATF color is milky or reddish brown, repair or replace the ATX, then go to the next step.
5 | VERIFY TROUBLESHOOTING OF DTC P0756 COMPLETED. • Make sure to reconnect all disconnected connectors. • Clear the DTC from the TCM memory using the WDS or equivalent. • Start the engine. • Warm up the ATX.
• Drive the vehicle in the D range and make sure that gears shift smoothly from 1GR to 5GR.
• Is the same DTC present?
Yes
Replace the TCM, then go to the next step.
(See TCM REMOVAL/INSTALLATION [JA5A-EL].)
No | Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [JA5A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [JA5A-EL].)
No | DTC troubleshooting completed.