#
DIAGNOSTIC MONITORING TEST RESULTS [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)

BME010200102211
• The purpose of this test mode is to confirm the result of OBD monitor diagnostic test results. The result values stored when particular monitor is completed are displayed. If the monitor is not completed, initial value is displayed.

TEST ID | Description | Related system
--- | --- | ---
10:02:11*1 | HO2S (Front, RH) lean-to-rich response time | HO2S
10:02:21*1 | HO2S (Front, LH) lean-to-rich response time
10:03:11*1 | HO2S (Front, RH) rich-to-lean response time
10:03:21*1 | HO2S (Front, LH) rich-to-lean response time
10:04:01 | HO2S (Front) rich/lean inversion voltage
10:04:02*1 | HO2S (Rear) rich/lean inversion voltage
10:05:01 | HO2S (Front) lean threshold voltage
10:06:01 | HO2S (Front) rich threshold voltage
10:11:11*1 | Front and HO2S (Rear) switching time ratio | TWC
10:11:21*1 | Front and HO2S (Rear) switching time ratio
10:41:00*2 | EGR pressure variation | EGR

  *1 :
European (L.H.D.) specs.
  *2 :
Australian, General (L.H.D. R.H.D.) specs.