#
FRONT A/C UNIT DISASSEMBLY/ASSEMBLY

BME071161130202

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Heater case (5)
2 | Cover
3 | Front evaporator (See Front Evaporator Assembly Note)
4 | Expansion valve
5 | Front heater core
6 | Airflow mode crank
7 | Airflow mode link
8 | Air mix link
9 | Air mix crank
10 | Thermosensor
11 | Heater case (4)
12 | Heater case (3)
13 | Heater case (2)
14 | Heater case (1)
15 | Airflow mode door
16 | Air mix door

## Front Evaporator Assembly Note

1. When assembling a new front evaporator, add a supplemental amount of ND-OIL8 compressor oil from the inlet.

Supplemental amount

  40 ml {40 cc, 1.4 fl oz}