#
EGR WATER COOLER REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME011620300W06

1. Disconnect the negative battery cable.

2. Remove the air cleaner. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the common rail. (See SUPPLY PUMP REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

4. Remove in the order indicated in the table.

1 | Air pipe (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)])
2 | EGR pipe
3 | EGR water cooler

5. Install in the reverse order of removal.