#
FRONT HEATER CORE INSPECTION

BME071161110201

1. Remove the front A/C unit. (See FRONT A/C UNIT REMOVAL/INSTALLATION.)

2. Remove the front heater core from the front A/C unit.

3. Inspect for cracks, damage, and coolant leakage.

  • If any problems are found, replace the front heater core.

4. Inspect for bent fins.

  • If any are bent, use a flathead screwdriver to straighten them.

5. Verify that the front heater core inlet and outlet are not distorted or damaged.

  • If they are distorted or damaged, repair them using pliers.