#
FRONT A/C UNIT OPERATION

BME071161133T01
• The front A/C unit which integrates the cooling and heater units has been adopted.

## Air Mix Door Operation

• The air mix door, installed in the front A/C unit, controls HOT or COLD position, depending on the position of the temperature control dial. As a result, airflow distribution changes, and the airflow temperature is controlled.

1 | Air mix door
2 | Front evaporator
3 | Front heater core
4 | Front A/C unit
5 | Front blower unit
6 | COLD
7 | HOT
8 | Cold air
9 | Warm air

## Airflow Mode Door Operation

• The airflow mode doors move to VENT, BI-LEVEL, HEAT, HEAT/DEF, or DEFROSTER position, depending on the position of the mode selector dial. As a result, airflow mode changes.

1 | Airflow mode door
2 | Front evaporator
3 | Front heater core
4 | Front A/C unit
5 | From blower unit
6 | To center and side vent
7 | To front and rear heat
8 | To defroster and side demister
9 | VENT
10 | BI-LEVEL
11 | HEAT
12 | HEAT/DEF
13 | DEFROSTER
14 | Cold air
15 | Warm air