| RIGHT-HAND REAR WIRING
H45/DG

#### 1107
CLUSTER SENSOR (YAW AND ACCELERATION SPEED)
TR4X4/RAD03

1 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY) | F041E
2 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | F041E
3 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL | F041E
4 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY) | F041E
5 | 0.5 | 4DS | - YAW SENSOR | F041E